StickShield v3 Change List
Saturday, June 2, 2018
6:06 PM
Feature Set
Raised gap and/or loopholes for string to tether both halves together (back of shell and bottom of guard?)
Branding/product name in circle around overhang?
OR gear-shaped overhang (work into tapering of higher pointy edges on guard)
"Squeeze-release" shell sides redesign?
Printing Layout (* = printed upside-down)
Perform test runs to find ideal notch + protrusion size pairings
Give support bridges wide bases for support
Guard Sections 
Button Zone:
j
Button Guard:
h
Upper Slope:
S
Overhang*:
h
Underhang:
j
Shell Sections
Core:
Correct for vertical leeway between joystick underside and surface of controller (about .4-.5mm)
Overhang*: 
C