Car Grip Mod
Monday, June 4, 2018
4:33 PM
Phone width: 76.25mm 
Mods width: 73.42mm 
Template width: 74.29mm
Magnet dia: 12mk depth: 5mm 
Distance below grip point: 22mm 
Grip innermost lip width: .56mm 
Grip innermost lip height: 1.77mm 
Shape is vert -> angle -> rounded corner -> vert
Grip height: 24.25mm 
Grip area depth: 13.5mm 
Mod width in grip zone: 67.25mm 
Adjustments:
Move the camera hole down 1mm 
Move the alignment nub up 1.25mm 
Move the entire bottom edge up 1.15mm
Make the smaller magnet holes go all the way through (so magnets can be ejected from backside)
Make outer camera hole taller (top edge shows in pics)
Make the origin of the camera hole .1-.2mm larger in diameter 
Move the upper magnet holes down 4mm 
Move the lower magnet holes down .5mm, inward 2mm 
Add a center cavity for ventilation / less material usage
Round edges of finger "grab" craters
Optional topside "hook" attachment to hang from mirror?