StickShield v2 Change List
Saturday, June 2, 2018
6:06 PM
Feature Set
Bottom-left two buttons shifted: .4mm away from center, .3mm left/down 
All button holes very slightly larger (.06mm?)
Slightly taller button section (or potentially only branding portion)
Added reinforcement for button section (S-shaped "branding?")
Inside tapering (slight) on lower pointy edges for shell and guard, higher pointy edges on guard only
Shift lock nubs, rests, and slits slightly further back (toward guard -- 0.3mm)
Raised gap and/or loopholes for string to tether both halves together (back of shell and bottom of guard?)
Branding/product name in circle around overhang?
OR gear-shaped overhang (work into tapering of higher pointy edges on guard)
"Squeeze-release" shell sides redesign?
Printing Layout (* = printed upside-down)
Several sections printed separately per piece, for better prints 
Some sections upside-down for reliable printing 
Notches and matching protrusions to line up sections of pieces 
All pieces and sections laid out from shortest to tallest with built-in paths/supports
Guard Sections 
Button Zone:
Square Z+ protrusion in center for Button Guard
Squared Z+ section from base of cone for Upper Slope
Two small square Z notches for Underhang
Button Guard: Square Z notch for Button Zone
Upper Slope:
Squared Z cutout near base of cone for Button Zone 
Two small square Z notches at top of cone for Overhang 
Overhang*: Two small square Z- protrusions for Upper Slope 
Underhang: Two small square Z+ protrusions for Button Zone 
Shell Sections
Core:
Inner edge only comes up to top of outer analog head rim 
Space for overhang has perfectly vertical cylinder inner walls (not part of cone)
Two square Z- notches for Overhang near the back
Overhang*: 
Cylindrical - no cone edges/walls, but straight up/down
Two square Z- protrusions for Core near the back