StickShield Measurements
Tuesday, May 29, 2018
9:43 PM
Joy-Con:
Primary depth: 14mm 
Analog cavity diameter: 15.36mm 
Analog base diameter: 10(.36?)mm 
Analog cavity "mote" width: 2.5mm
Gap - Joy-Con surface up to bottom of analog stick head: 3.35mm 
Step-down from Joy-Con surface to surface of analog cavity: 1.44mm 
Analog head SAFE diameter: 15.10mm (varies - up to .1mm smaller)
Analog head outer rim height: 3.2mm 
Analog head total height: 4.15mm 
ABXY button diameter: Varies - 7.27mm max
Distance from analog cavity edge to nearest ABXY button edge - both Joy-Con: 9.1mm 
Button array height: 22mm 
Button array width: 22.7-22.8mm 
Button depth from Joy-Con surface: 1.52mm
Theoretical Mod Measurements:
Maximum added radius (from analog cavity): 5.5mm 
Space between analog head edge and head's raised center surface for a 1mm-thick "protective rim": 2.9mm 
An extension of the thinner, straight component to cover/prevent accidental pressing of the ABXY buttons
Lock slit length: 9mm
Lock slit depth: 0.5mm
Lock section depth: 0.6mm
Lock section width: 3mm
Lock nub height: 1.9mm
Lock nub width: 1.3mm
Lock nub depth: 0.7mm
Lock nub seat depth: 1mm
Lock nub seat height: 1.3mm
Lock nub seat width: 1.9mm
Z: 1.5
Back toward guard: -1.45
In toward center: -2.67