Quest HP Mount
Tuesday, May 28, 2019
12:41 PM
Essential measurements:
- Avg. distance from middle of swivel mount to inner speaker edge: 22.7mm
"" to inner housing edge: 11.3mm (read: Is the distance from clip's outer face to center of rail depth)
NOTE: Best fwd. rotation we can do, then, is approx. 45 degrees.
- Rail thickness: OG .85mm, max 1mm
- Rail gap width TIGHT: OG 4.08mm, but maths suggest accurate answer is 4mm
- Rail gap width LOOSE: 4.6mm
- Rail gap width ENTRYPOINT: 11.5mm
- Swivel mount diameter: 13.4mm
- (In case needed) Est. length of wider inner swivel mount section: 7.65mm
- Swivel mount upper half depth: 2.2mm (read: will be depth of guard rail)
- Rail width (front or back): 4.5mm
- Total rail width: 13mm
- Headphone speaker diameter: 47.65mm
- Inflexible audio cable protrusion length: 8.6mm
Plus addtl. Cable space: 12.6mm
Total distance from bottom clip edge to center of swivel mount: 60.25mm
Above but calculated: 36.425mm
Clip outer face thickness: 4.21mm
Snap swivel horizonal multiplier: 30x
Snap swivel vertical multiplier: 10x
Build measurements:
Swivel plate
Width: 13.4 + 0.6 + 4.5 = 18.5mm
Depth: 11.8mm (assuming rails will be 1mm thick)
Snap swivel
Head Diameters:
Base: .24 * 30 = 7.2mm
Upper: .28 * 30 = 8.4mm
Top: .2 * 30 = 6mm
Head Gap width: .06 * 30 = 1.8mm
Head Heights:
Base: 2.3mm
Trans. To upper: .2mm
Upper: .6mm
Trans. To top: .4mm
Socket diameters:
Center: .274 * 30 = 8.22mm
Outer; upper shield: 9.72mm
Socket heights:
Center: 2mm
Outer: .25mm