Joy-Mod Measurements
Tuesday, May 29, 2018
9:43 PM
Joy-Con:
Primary depth: 14mm 
Moto Z2 Play:
Primary depth: 6.2mm 
W/Camera Hump: 9mm 
Height: 156mm 
Space beneath camera: 119.3mm 
Magnet center locations on mod (9):
X: Center, Y: 11.6 down from top (as close to cam hump as possible)
X: 15.28 from right, Y: 16.3 from top 
X: 13.85 from left, Y: 17.1 from top 
X: 17 from right, Y: 43.5 from top 
X: 15 from right, Y: 65 from top 
X: 13.4 from right, Y: 35.8 from bottom
X: 20.25 from right, Y: 19 from bottom
X: 20.25 from left, Y: 19 from bottom
X: 10.1 from left, Y: 12.2 from bottom
Ideal magnet diameter: 8mm
Magic-NS:
Depth: 8.8mm 
Probable casing-less depth: 6.1mm 
Actual: 6.85mm
Theoretical Mod Measurements:
Perfect depth (added to phone to match Joy-Con depth): 7.8mm 
Total depth allotted to outer+inner casing walls, given ideal vs. board depth: .95mm 
Ideal minimum depth of each wall: 1.4mm
Speaker mod depth (for comparison): 14.85mm 
New ideal depth: 9.65mm
Vertical space in mod needed for wireless adapter assembly, including cord bend when packed-up: 108.8mm 
Considered peripherals:
Thumb drive total depth: 8.5mm 
Depth of USB portion: 
Length: 19.15mm