StickShield v4 Change List
Saturday, June 2, 2018
6:06 PM
Feature Set
Raised gap and/or loopholes for string to tether both halves together (back of shell and bottom of guard?)
Branding/product name in circle or slope around overhang?
"X Helmet" and/or diamond styling?
"Hook" design
Guard connects to Shield along outer edge (near Joy-Con outside) as opposed to center
Shield backside faces top of Joy-Con (shield rotated 180 degrees)
Shield opening (for sliding analog in) is directly above top of Guard
Ensure enough of a gap to slide StickShield under the analog stick from outer edge, then down
"Three-triangle" arrow design(s) along edges to indicate motion needed to attach StickShield
Bring in under-shield walls by at least .5mm on each side (hole diameter reduced by 1mm)
Under-shield walls to have gradual overhang slope up about 75-80% of the way, then reverse that slope to meet topside
Increase height of analog under-shield by ~.2mm (for sturdier connection, prevent analog click & slight tilt) - potentially only to front portions of the "fork," depending on design
Widen each under-shield fork point to not fall inside the analog mote at the tips. Gives more anti-tilt support.
Slight outward, downward slope on top at tip of each under-shield fork point
Quarter-circular curve on top at tip of each shield wall fork point
Inner-shield rim overhang slope to begin at least 1.2mm lower, come in at least 1mm more
Some means of attaching to the Joy-Con rail and/or another StickShield for easy stowing?