Envelope-based internal controller.