A bank of 8 delay lines with filtered feedback.