Cup Holder Assistant
Tuesday, June 5, 2018
5:08 PM
Measurements 
Base max length: 137.5mm 
Base min length: 136.5mm (side curved slightly)
Thinner base section length (below): 129.18mm
Curve-to-top span from top corner of side: 6.61mm
Span of relatively flat portion of sides: 53.63mm 
Span of lower transition to thinner base edge: 5.86mm 
Span of thinner base section sides (where bottom edge meets raised lip): 12.43mm
Span (distance) from lower curve of raised lip to upper (the "hilltop"): 19.83mm 
Depth of raised lip: 1.95mm 
Greatest distance from holder base to top of wall: 56.28mm 
Same section - to bottom of wall: 29.5mm 
Same section - total wall height: 26.78mm 
Front section - to top of wall: 50.59mm 
Back section - to top of wall: 38.28mm
Rough max upper diameter of walls: 88.5mm 
Rough min diameter of walls (at bottom of wall): 78.22mm
Depth of base plate: 3.3mm 
Distance inward from wider base section outer edge to underside support: 10.9mm 
"" - but for thinner base section: 7.6mm 
Y-span from back lip to thinner base section's X-axis support: 6.1mm 
Said support's thickness: 1.55mm
Minimum resting clearance beneath base plate: 8.7mm